BIOS Update via UEFI Shell 

Preparation:
	1.	Prepare a USB drive and format it as FAT32
	2.	Extract the BIOS update zip file to the root directory of the USB drive:
	3.	Ensure the USB drive also contains:
	•	EFI/BOOT/BOOTX64.EFI (UEFI Shell)


Update Steps:
	1.	Insert the USB drive into the system
	2.	Power on and enter the Boot Menu (Delete key)
	3.	Select the USB drive to boot
	4.	The system will automatically enter UEFI Shell and start the BIOS update process


Important Notes:
	•	Do NOT power off the system during the update
	•	The system will reboot automatically after completion
	•	If the update does not start automatically, please check:
	•	USB is formatted as FAT32
	•	Files are in the root directory (not inside a folder)